Process “Add New Client”

New Client has configuration file with the following predefined information:

1. Client ID
2. Server IP
3. In case if VPN is implemented – Server certificate (not a part of config file)

Once a day, Client sending confirmation request to server

Stop

Server accepting connection and sending back approval

Client Initiate connection with the server

Start

Process “Keep Alive”

Every minute, Server sending to each Client request “Keep Alive”